# Version 0.4 assembly verification checklist

- [ ] No unresolved hard interference in cruise-deployed arrangement
- [ ] Solar and radiator deployment paths clear structural and habitation envelopes
- [ ] Thruster plume cones clear radiators, solar arrays and Skimmer
- [ ] Ring sectors form two closed 12-position circular patterns
- [ ] Rotating-ring subassemblies remain kinematically independent of the fixed spine
- [ ] All replaceable pods have removal corridors
- [ ] Skimmer capture and separation path is unobstructed
- [ ] Component names comply with the AST part-number scheme
- [ ] All WAVE links resolve to the controlled master skeleton
- [ ] NX dry mass agrees with `component_mass_properties.csv` to within the documented modelling maturity
- [ ] CG remains inside the preliminary ±2.5 m axial control envelope for published loading cases
- [ ] Analysis reference sets suppress nonessential detail
