{
  "version": "0.5.0",
  "required_files": 19,
  "nodes": 222,
  "elements": 580,
  "remote_mass_kg": 42800.0,
  "static_cases": 7,
  "first_supported_screening_frequency_Hz": 0.130787401424204,
  "governing_displacement_case": "LC-STR-05",
  "governing_displacement_mm": 105.14727698319136,
  "status": "PASS"
}
