{
  "status": "screening_only",
  "solver": "custom linear 3-D Euler-Bernoulli frame",
  "nodes": 222,
  "elements": 580,
  "structural_tube_mass_kg": 7742.282,
  "approximate_total_lumped_mass_kg": 50542.28253244922,
  "static_cases": [
    {
      "load_case_id": "LC-STR-01",
      "support_model": "aft_fixed",
      "result_source": "Independent Python Euler-Bernoulli frame screening",
      "max_translation_mm": 0.8095171570870019,
      "critical_node_id": 179,
      "max_screening_von_mises_MPa": 3.9530093569420948,
      "critical_element_id": 570,
      "minimum_yield_factor": 127.24482908613771,
      "minimum_member_euler_factor": 328.61679514151746
    },
    {
      "load_case_id": "LC-STR-02",
      "support_model": "aft_fixed",
      "result_source": "Independent Python Euler-Bernoulli frame screening",
      "max_translation_mm": 13.787658028944621,
      "critical_node_id": 214,
      "max_screening_von_mises_MPa": 43.134828549406755,
      "critical_element_id": 563,
      "minimum_yield_factor": 11.661110451009732,
      "minimum_member_euler_factor": 195.04313402086396
    },
    {
      "load_case_id": "LC-STR-03",
      "support_model": "aft_fixed",
      "result_source": "Independent Python Euler-Bernoulli frame screening",
      "max_translation_mm": 0.17640517527317418,
      "critical_node_id": 176,
      "max_screening_von_mises_MPa": 4.428268725973788,
      "critical_element_id": 537,
      "minimum_yield_factor": 113.5884091788917,
      "minimum_member_euler_factor": 18.025775221861355
    },
    {
      "load_case_id": "LC-STR-04",
      "support_model": "aft_fixed",
      "result_source": "Independent Python Euler-Bernoulli frame screening",
      "max_translation_mm": 6.609803314527801,
      "critical_node_id": 219,
      "max_screening_von_mises_MPa": 2.9767766242263374,
      "critical_element_id": 200,
      "minimum_yield_factor": 168.97472114849378,
      "minimum_member_euler_factor": 15.530208906833764
    },
    {
      "load_case_id": "LC-STR-05",
      "support_model": "aft_fixed",
      "result_source": "Independent Python Euler-Bernoulli frame screening",
      "max_translation_mm": 105.14727698319135,
      "critical_node_id": 189,
      "max_screening_von_mises_MPa": 9.941003805706382,
      "critical_element_id": 489,
      "minimum_yield_factor": 50.59851196428127,
      "minimum_member_euler_factor": 27.31120121979528
    },
    {
      "load_case_id": "LC-STR-06",
      "support_model": "aft_fixed",
      "result_source": "Independent Python Euler-Bernoulli frame screening",
      "max_translation_mm": 13.787671493973484,
      "critical_node_id": 214,
      "max_screening_von_mises_MPa": 43.13481408491083,
      "critical_element_id": 557,
      "minimum_yield_factor": 11.661114361356585,
      "minimum_member_euler_factor": 18.0257225356448
    },
    {
      "load_case_id": "LC-STR-07",
      "support_model": "aft_fixed",
      "result_source": "Independent Python Euler-Bernoulli frame screening",
      "max_translation_mm": 52.8225877180624,
      "critical_node_id": 219,
      "max_screening_von_mises_MPa": 11.151134876479341,
      "critical_element_id": 9,
      "minimum_yield_factor": 45.1075164610338,
      "minimum_member_euler_factor": 42.28927138294497
    }
  ],
  "supported_modal_frequencies_Hz": [
    0.13078740142420406,
    0.15659762020582738,
    0.15659904416592052,
    0.16996982102983432,
    0.17749884705362573,
    0.17750294027565675,
    0.19598863500694386,
    0.2219275924973127,
    0.2870794700934411,
    0.29745535594973954,
    0.29850043589492964,
    0.3830616852908203
  ],
  "limitations": [
    "Ideal rigid beam joints",
    "No shear deformation or warping",
    "Simplified nearest-node placement for subsystem mass",
    "Approximate positive rotary lumped mass",
    "No contact, geometric nonlinearity, joint flexibility or imperfections",
    "ANSYS Mechanical results are required for final portfolio claims"
  ]
}
