# Manufacturing verification checklist

- [ ] Design revision matches the released drawing.
- [ ] Material and stock certificate recorded.
- [ ] MCS and work offset independently checked.
- [ ] Tool and holder assemblies match the physical setup.
- [ ] Fixture and clamp envelopes included in simulation.
- [ ] All rapid moves remain clear of stock and fixtures.
- [ ] IPW is transferred correctly between setups.
- [ ] Finish stock is intentional and documented.
- [ ] Posted code matches the approved controller/post.
- [ ] Dry run and first-off inspection completed.
- [ ] Final inspection record attached.
- [ ] Deviations and concessions documented.
