# Version 0.2 Verification Record

| ID | Verification item | Evidence | Result |
|---|---|---|---|
| V02-001 | Core station range is −21,000 to +21,000 mm | `station_table.csv` | Pass |
| V02-002 | Ring outer diameter is 26,000 mm | expressions and geometry report | Pass |
| V02-003 | Ring centres are at STA_30 and STA_40 | station and coordinate tables | Pass |
| V02-004 | Solar tip-to-tip span is 58,000 mm | expressions and neutral geometry | Pass |
| V02-005 | Six equal propulsion interfaces exist | `interface_points.csv` | Pass |
| V02-006 | Skimmer dock is at STA_70 | interface and station tables | Pass |
| V02-007 | Neutral GLB, STL and OBJ exports exist | release manifest | Pass |
| V02-008 | NX native-build procedure exists | `nx_build_tutorial.md` | Pass |
| V02-009 | Native `.prt` is not falsely claimed | README and release notes | Pass |
| V02-010 | Validation script completes | validation output | Pass |
