{
  "status": "screening_only",
  "solver": "custom linear 3-D Euler-Bernoulli frame",
  "nodes": 222,
  "elements": 648,
  "structural_tube_mass_kg": 10423.430670108912,
  "approximate_total_lumped_mass_kg": 53223.43067010891,
  "static_cases": [
    {
      "load_case_id": "LC-STR-01",
      "support_model": "aft_fixed",
      "result_source": "Independent Python Euler-Bernoulli frame screening",
      "max_translation_mm": 0.6965874615230333,
      "critical_node_id": 219,
      "max_screening_von_mises_MPa": 2.6707727047580945,
      "critical_element_id": 569,
      "minimum_yield_factor": 188.33500848046117,
      "minimum_member_euler_factor": 8.101620246518904
    },
    {
      "load_case_id": "LC-STR-02",
      "support_model": "aft_fixed",
      "result_source": "Independent Python Euler-Bernoulli frame screening",
      "max_translation_mm": 0.2148503461176776,
      "critical_node_id": 176,
      "max_screening_von_mises_MPa": 1.073615687592714,
      "critical_element_id": 75,
      "minimum_yield_factor": 468.5102926614627,
      "minimum_member_euler_factor": 184.48557719983637
    },
    {
      "load_case_id": "LC-STR-03",
      "support_model": "aft_fixed",
      "result_source": "Independent Python Euler-Bernoulli frame screening",
      "max_translation_mm": 0.14604598362720486,
      "critical_node_id": 174,
      "max_screening_von_mises_MPa": 2.7361626727971067,
      "critical_element_id": 505,
      "minimum_yield_factor": 183.83409912020926,
      "minimum_member_euler_factor": 11.815516372270194
    },
    {
      "load_case_id": "LC-STR-04",
      "support_model": "aft_fixed",
      "result_source": "Independent Python Euler-Bernoulli frame screening",
      "max_translation_mm": 2.795165605791783,
      "critical_node_id": 219,
      "max_screening_von_mises_MPa": 1.2835969915645227,
      "critical_element_id": 9,
      "minimum_yield_factor": 391.86754355579654,
      "minimum_member_euler_factor": 24.801469415115825
    },
    {
      "load_case_id": "LC-STR-06",
      "support_model": "aft_fixed",
      "result_source": "Independent Python Euler-Bernoulli frame screening",
      "max_translation_mm": 0.30315213353710463,
      "critical_node_id": 199,
      "max_screening_von_mises_MPa": 2.73810288048097,
      "critical_element_id": 529,
      "minimum_yield_factor": 183.70383508440122,
      "minimum_member_euler_factor": 11.641855199973389
    },
    {
      "load_case_id": "LC-STR-07",
      "support_model": "aft_fixed",
      "result_source": "Independent Python Euler-Bernoulli frame screening",
      "max_translation_mm": 22.8695049967966,
      "critical_node_id": 222,
      "max_screening_von_mises_MPa": 7.530079304234314,
      "critical_element_id": 9,
      "minimum_yield_factor": 66.79876528221331,
      "minimum_member_euler_factor": 7.9002920285570815
    },
    {
      "load_case_id": "LC-STR-08",
      "support_model": "aft_fixed",
      "result_source": "Independent Python Euler-Bernoulli frame screening",
      "max_translation_mm": 1.8464527340647814,
      "critical_node_id": 208,
      "max_screening_von_mises_MPa": 0.8750870212595403,
      "critical_element_id": 240,
      "minimum_yield_factor": 574.7999773508425,
      "minimum_member_euler_factor": 13.919623471075411
    },
    {
      "load_case_id": "LC-STR-09",
      "support_model": "aft_fixed",
      "result_source": "Independent Python Euler-Bernoulli frame screening",
      "max_translation_mm": 3.486900488908973,
      "critical_node_id": 181,
      "max_screening_von_mises_MPa": 0.6129629680606593,
      "critical_element_id": 22,
      "minimum_yield_factor": 820.6042227827093,
      "minimum_member_euler_factor": 20.873684415750933
    }
  ],
  "supported_modal_frequencies_Hz": [
    0.1964088051840446,
    0.19644133264213973,
    0.2213052556499484,
    0.22133270851902045,
    0.22990069165409538,
    0.25877996892656085,
    0.30563870170112994,
    0.4011941565582085,
    0.4025482045274537,
    0.4029063455552414,
    0.44029449537109216,
    0.44660093940522827
  ],
  "limitations": [
    "Ideal rigid beam joints",
    "No shear deformation or warping",
    "Simplified nearest-node placement for subsystem mass",
    "Approximate positive rotary lumped mass",
    "No contact, geometric nonlinearity, joint flexibility or imperfections",
    "ANSYS Mechanical results are required for final portfolio claims"
  ]
}
