# ASTERION NX MASTER MODEL EXPRESSIONS — VERSION 0.1
# Units should be assigned explicitly in NX.

vehicle_length = 42000 mm
spine_length = 42000 mm
spine_outer_radius = 900 mm
spine_truss_radius = 1200 mm

ring_outer_diameter = 26000 mm
ring_outer_radius = ring_outer_diameter / 2
ring_occupied_radius = 12000 mm
ring_width = 3200 mm
ring_depth = 2800 mm
ring_sector_count = 12
ring_sector_angle = 360 deg / ring_sector_count
ring_spacing = 5000 mm
ring_rotation_speed = 4.3 rpm
ring_target_gravity = 0.25

solar_wing_count = 4
solar_wing_length = 20500 mm
solar_wing_width = 4200 mm
solar_hinge_offset = 8500 mm
solar_deployed_span = 58000 mm

radiator_count = 6
radiator_length = 9000 mm
radiator_width = 2800 mm
radiator_deploy_angle = 70 deg

propulsion_pod_count = 6
thrusters_per_pod = 2
thruster_cant_angle = 3 deg
propulsion_frame_station = -16000 mm

skimmer_length = 8000 mm
skimmer_width = 5500 mm
skimmer_height = 2100 mm
skimmer_dock_station = 21000 mm

module_pitch = 2500 mm
primary_docking_diameter = 1600 mm
service_tunnel_diameter = 1200 mm

# Station coordinates along +X
sta_00 = -21000 mm
sta_10 = -16000 mm
sta_20 = -8000 mm
sta_30 = -2500 mm
sta_40 = 2500 mm
sta_50 = 9000 mm
sta_60 = 15000 mm
sta_70 = 21000 mm
